From fc3ec276bc47d208beaf2d7602258e13de1385a1 Mon Sep 17 00:00:00 2001
From: Benedikt Peetz <benedikt.peetz@b-peetz.de>
Date: Mon, 16 Sep 2024 18:41:09 +0200
Subject: chore(references): Add testing data

---
 .../content/05_aufbau/figures/threeDModel.tex      | 74 ++++++++++++++++++++++
 1 file changed, 74 insertions(+)
 create mode 100644 reference/C_Facharbeit_komplett/content/05_aufbau/figures/threeDModel.tex

(limited to 'reference/C_Facharbeit_komplett/content/05_aufbau/figures/threeDModel.tex')

diff --git a/reference/C_Facharbeit_komplett/content/05_aufbau/figures/threeDModel.tex b/reference/C_Facharbeit_komplett/content/05_aufbau/figures/threeDModel.tex
new file mode 100644
index 0000000..fe3aeed
--- /dev/null
+++ b/reference/C_Facharbeit_komplett/content/05_aufbau/figures/threeDModel.tex
@@ -0,0 +1,74 @@
+%! TEX root = ../../../facharbeit.tex
+% LTeX: language=de-DE
+
+% \imagelabelset{
+%   coarse grid color = red,
+%   fine grid color = gray,
+%   image label font = \sffamily\bfseries\small,
+%   image label distance = 2mm,
+%   image label back = black,
+%   image label text = white,
+%   coordinate label font = \sffamily\bfseries\scriptsize,
+%   coordinate label distance = 2mm,
+%   coordinate label back = black,
+%   coordinate label text = white,
+%   annotation font = \normalfont\small,
+%   arrow distance = 1.5mm,
+%   border thickness = 0.6pt,
+%   arrow thickness = 0.4pt,
+%   tip size = 1.2mm,
+%   outer dist = 0.5cm,
+% }
+% \let\tikzset\imagelabelset
+
+\begin{figure}[h]
+	\center
+	\begin{tikzpicture}
+		% Grid
+		% \draw[very thin, draw=gray, step=0.5] (0,0) grid (7,7);
+		% \draw[thin, draw=\maingridcolor, xstep=0.1, ystep=0.5] (0,0) grid (7,7);
+		% \foreach \x in {0,1,...,7} {
+		% 		\node [anchor=north] at (\x,0) {\tiny \x};
+		% 	}
+		% \node [anchor=north] at (1,0) {\tiny 1};
+		%
+		% \foreach \y in {0,1,...,7} {
+		% 		\node [anchor=east] at (0,\y) {\tiny \y};
+		% 	}
+		% \node [anchor=east] at (0,1) {\tiny 1};
+
+
+		\node[] (kuvette) at (1,0.5) {Küvette};
+		\node[] (laser) at (-0.5,4) {Laser};
+		\node[] (kollimationsLinse) at (2.5,3.5) {Kollimations Linse};
+		\node[] (planoKonvexeFokusLinse) at (1,5) {Plano-konvexe Fokus Linse};
+		\node[] (smartphoneHalterung) at (6,5) {Smartphone-Halterung};
+		\node[] (abnehmbarerGitterHalter) at (6,0) {abnehmbarer Gitter Halter};
+		\node[] (schieneFürLinsenHalter) at (3,-1) {Schiene für Linsen/Halter};
+		\begin{scope}[xshift=0cm]
+			\node[anchor=south west,inner sep=0] (image) at (0,0) {\includegraphics[width=0.9\columnwidth]{figures/3d_raman_spectrometer_model_trans.png}};
+			\begin{scope}[x={(image.south east)},y={(image.north west)}]
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (kuvette) to (0.3,0.45);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (laser) to (0.2,0.6);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (kollimationsLinse) to (0.42,0.5);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (planoKonvexeFokusLinse) to[out=0, in=90] (0.64,0.6);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (smartphoneHalterung) to (0.7,0.7);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (abnehmbarerGitterHalter) to (0.8,0.76);
+				\draw [-{Circle[fill=black, length=\tipsize, width=\tipsize]}, black, line width = 0.4pt] (schieneFürLinsenHalter) to (0.6,0.34);
+			\end{scope}
+		\end{scope}
+	\end{tikzpicture}
+
+	% \draw[annotation left = {Küvette at 0.8}] to (0.39,0.45);
+	% \draw[annotation left = {Laser at 0.5}] to (0.2,0.6);
+	% \draw[annotation below = {Kollimations Linse at 0}] to (0.42,0.5);
+	% \draw[annotation below = {Plano-konvexe Fokus Linse at 0.6}] to (0.64,0.6);
+	% \draw[annotation above = {Smartphone-Halterung at 0}] to (0.7,0.7);
+	% \draw[annotation above = {abnehmbarer Gitter Halter at 0.6}] to (0.76,0.7);
+	% \draw[annotation right = {Schiene für Linsen/Halter at 0.5}] to (0.6,0.34);
+	\caption{
+		Das 3d Modell für den Aufbau.
+		\Vref{chap:Links} beinhaltet einen Link zu dem \texttt{OpenSCAD} Quellcode.
+		\Vref{fig:threeDModelBigger} zeigt das Bild in voller Größe.
+	}\label{fig:threeDModel}
+\end{figure}
-- 
cgit 1.4.1

